

RECATIVE COLD DYES

|  |  |
| --- | --- |
| **Reactive Cold Dyes** | **FASTNESS PROPERTIES** |
| Light | Washing | Perspiration | Hypochlorite | Dischargeability |
| Reactive Red M5BReactive Red - 2 |   | 4-5 | 4-5 | 3-4 | 1 | P |
| Reactive Red M8BReactive Red - 11 |   | 4-5 | 4-5 | 2 | 4 | P |
| Reactive Magenta MBReactive Violet - 13 |   | 4-5 | 5 | 4-5 | 1 | F |
| Reactive Orange M2RReactive Orange - 4 |   | 5 | 5 | 4 | 4 | P |
| Reactive Orange M2RJ  |   | 3-4 | 4 | 4 | 4-5 | P |
| Reactive Gol. Yellow MRReactive Yellow - 44 |   | 5 | 4-5 | 4 | 1 | P |
| Reactive Yellow MR EX H/CReactive Yellow - 44 |   | 5 | 4-5 | 4 | 1 | P |
| Reactive Yellow M3RReactive Yellow - 36 |   | 6 | 5  | 4 | 2 | G |
| Reactive Yellow M4RReactive Orange - 14 |   | 5 | 4-5 | 4 | 1 | P |
| Reactive Yellow M8GReactive Yellow - 86 |   | 6 | 4-5 | 4-5 | 1 | G |
| Reactive Yellow M4GReactive Yellow - 22 |   | 6 | 4 | 5 | 1 | G |
| Reactive Yellow MGRReactive Yellow - 7 |   | 6 | 5 | 4-5 | 4-5 | P |
| Reactive Violet C4RReactive Violet - 12 |   | 4 | 3 | 4 | 1 | P |
| Reactive Violet C2RReactive Violet - 14 |   | 3-4 | 3  | 4 | 1 | P |
| Reactive Blue MRReactive Blue - 4 |   | 6 | 5 | 5 | 2 | P |
| Reactive Blue M2RReactive Blue - 81 |   | 6 | 5 | 4-5 | 1 | P |
| Reactive Blue M2R H/CReactive Blue - 81 |   | 6 | 5 | 4-5 | 1 | P |
| Reactive Navy Blue M3RReactive Blue - 9 |   | 5 | 4-5 | 3 | 3 | P |
| Reactive Blue M4GD H/CReactive Blue - 168 |   | 6 | 5 | 3-4 | 2 | P |
| Reactive Tur. Blue MGNReactive Blue - 140 |   | 6 | 4 | 4 | 2-3 | P |
| Reactive Tur. Blue Ha5GReactive Blue - 71 |   | 6 | 3-4 | 4-5 | 3-4 | P |